Station ID:

US Robotics V-everything

UNAVCO Number:

Model Number:

Serial Number:

Dip switches:

Switch #	Function	ON	OFF	Function
1	DTR always ON
DTR Normal
2	Numeric Results Code
Verbal results Code
3	Display Results Code
Suppress results code
4	No Echo
Echo Offline command
5	Suppress auto answer
Auto Answer on ring
6	Carrier Detect override
Normal Carrier Detect
7	Results Code Orig
Display all results code
8	Enable AT command set
Disable at command set
9	No disconnect with +++
Disconnect with +++
10	Load &F0 settings
Load NVRAM defaults

ATI4:

ATI5:

What is the modems serial port connected to?

Cable Information:

Mgetty information /etc/inittab:

Does the modem access an ISP?

Phone number:

User name:

Password:

/etc/wvdial.conf:

Additional Notes:

Permanent Station Installation Information

- 1 -

Station ID:

jimg

2004-01-21

UNAVCO